2436P

**Sequential mechanical basin mixer**

Reference: 2436P

Specification Description

Wall-mounted 90° sequential basin mixer.

Open and closing on cold water.

Flat swivelling under spout L. 200mm with hygienic flow straightener

suitable for fitting a BIOFIL terminal filter.

Securitouch thermal insulation prevents burns.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume

(reduces bacterial development).

Flow rate limited to 5 lpm at 3 bar.

Chrome-plated brass body.

Non-manual contact operation with Hygiene control lever L. 200mm.

Supplied with 2 in-line STOP/CHECK connectors ideal for hospitals.