DELABIE_C100M35379DER15

**TEMPOMATIC Mix 4 electronic mixer**

Reference: 493400

CCTP description

Wall-mounted electronic basin mixer:

230/6V recessed mains supply.

Reduced-stagnation solenoid valve and electronic unit integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.5 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated metal body L. 160mm.

Cap fixed in place by 2 concealed screws.

Stopcocks.

Wall-mounted.

Recessed inlets ½”.

Anti-blocking security.

Side temperature control with adjustable maximum temperature limiter.

10-year warranty.

Provisional availability 2nd half 2019, please contact the sales office to check availability.