DELABIE_C100M35511906W

**Be-Line grab bar Ø 35mm, 600mm**

Reference: 511906W

Specification Description

Be-Line grab bar Ø 35mm, for people with reduced mobility.

Aluminium tube, 600mm centre-to-centre, 3mm thick. Solid aluminium fixing points.

For use as a handrail or grab bar for WCs, showers or baths.

Rounded profile Ø 35mm with ergonomic flat front face that prevents rotation for an optimal grip.

Matt white epoxy coated aluminium finish provides a good visual contrast with the wall.

Uniform surface for easy maintenance and hygiene.

38mm gap between the bar and the wall:

minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings.

Supplied with stainless steel screws Ø 8 x 70mm for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.