DELABIE_C100M35511920C

**Be-line lift-up shower seat**

Reference: 511920C

Specification Description

Be-line removable lift-up for people with reduced mobility.

Large model.

Removable: easy to remove with anti-theft locking system. Reduces the number of shower seats in a facility, allowing installation only when required e.g. hotels or hospitals providing short-term accommodation for people with reduced mobility.

Retained in upright position. Slowed down descent.

Solid, reinforced seat made from high strength polymer which can be installed, without a supporting leg, on any suitable wall.

Suitable for intensive use in public places or the healthcare sector.

Non-slip surface.

Metallised anthracite epoxy coated aluminium provides a good visual contrast with the wall.

Solid aluminium mounting bracket.

5 concealed fixing points.

Supplied with stainless steel screws Ø 8 x 70mm for concrete walls.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Dimensions: 455 x 450 x 90mm.

Folded dimensions: 85 x 470mm.

10-year warranty. CE marked.