DELABIE_C100M355160P1

**Drop-down rail, Ø 33.7mm, L. 650mm**

Reference: 5160P1

Specification Description

Drop-down grab bar Ø 33.7mm, for PRM.

In the lowered position use as a grab bar, for standing up and assisting movement. For WCs or showers. Allows side access in the raised position.

Dimensions: 650 x 290 x 110mm.

Bacteriostatic 304 stainless steel tube.

Stainless steel with UltraPolish bright polished finish, uniform non-porous surface for easy maintenance and hygiene.

Visible fixings with a 304 stainless steel cover plate, 2.5mm thick.

Supplied with stainless steel screws for concrete walls.

Tested to over 200kg. Maximum recommended user weight 135kg.