745250

**TEMPOSTOP**

Reference : 745250

CCTP description

Deck-mounted time flow basin tap:

Time flow ~7 sec.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.5 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated solid brass body with Ø 15mm conical inlet.

Fixing with back-nut.