79230015

**SECURITHERM shower panel**

Reference: 79230015

CCTP description

Time flow thermostatic shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet via in-line stopcocks and conical Ø 15mm inlets.

SECURITHERM thermostatic mixer.

Adjustable temperature: from cold water to 41°C using the temperature control.

Anti-scalding safety: automatic shut-off if cold or hot water supply fails.

Thermal shocks are possible.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

Concealed fixings.

Filters and non-return valves.