DELABIE_C100M35H960015L

**SECURITHERM thermostatic basin mixer**

Reference: H960015L

Specification Description

Deck-mounted SECURITHERM sequential thermostatic basin mixer H. 85mm L. 120mm, without pop-up waste.

Anti-scalding failsafe: hot water shuts off immediately if cold water supply fails.

Securitouch thermal insulation prevents burns.

No non-return valves on the inlets.

Straight spout with a hygienic flow straightener, no build-up of impurities and withstands thermal shocks.

Scale-resistant thermostatic sequential cartridge for single control adjustment of flow rate and temperature.

Adjustable temperature from cold water up to 40°C with maximum temperature limiter set at 40°C and the option to carry out thermal and chemical shocks.

Spout and body with smooth interiors and low water volume.

Flow rate regulated at 7 lpm.

No manual contact thanks to Hygiene control lever L. 100mm.

PEX flexibles supplied with stopcocks in chrome-plated brass Ø 15mm.

Reinforced fixing via 2 stainless steel rods.

10-year warranty.

Also available with copper tubes.