H9605610

**SECURITHERM BIOCLIP thermostatic basin mixer**

Reference : H9605610

CCTP description

Deck-mounted SECURITHERM BIOCLIP sequential thermostatic basin mixer H. 85mm L. 120mm, without pop-up waste.

Can be removed entirely for cleaning/disinfection.

Anti-scalding failsafe: hot water shuts off immediately if cold water supply fails (and vice versa).

Securitouch thermal insulation prevents burns.

No non-return valve.

Straight spout with a hygienic flow straightener, no build-up of impurities and withstands thermal shocks.

Scale-resistant thermostatic sequential cartridge for single control adjustment of flow rate and temperature.

Adjustable temperature from cold water up to 40°C with maximum temperature limiter set at 40°C and the option to carry out thermal and chemical shocks.

Spout and body with smooth interior and low water volume.

Flow rate limited to 7 lpm at 3 bar.

No manual contact thanks to Hygiene control lever L. 146mm.

Supplied with copper tails and stopcocks in chrome-plated brass Ø 15mm.

Reinforced fixing via 2 stainless steel rods.