DELABIE_C100M35H9611P

**SECURITHERM BIOCLIP thermostatic sink mixer**

Reference: H9611P

Specification Description

Wall-mounted SECURITHERM thermostatic sequential sink mixer with removable BIOCLIP spout.

Comes with 2 stainless steel BIOCLIP spouts (ref. 20003) L. 135mm Ø 28mm for complete internal cleaning/descaling.

Can be replaced with 10 BIOFIL filter spouts for immediate protection against waterborne infections, or 15 disposable Hostaform® spouts (recyclable) with star shaped flow straightener.

Anti-scalding failsafe: hot water shuts off immediately if cold water supply fails.

Securitouch thermal insulation prevents burns.

No non-return valves on the inlets.

Scale-resistant thermostatic sequential cartridge for single control temperature and flow-rate adjustment.

Adjustable temperature from cold water to 40°C with maximum temperature limiter set at 40°C.

Chemical and thermal shocks can be carried out.

Smooth body and spout interiors, with low water volume (reduces niches where bacteria can develop).

Flow rate regulated at 7 lpm.

No manual contact thanks to Hygiene control lever L. 146mm.

Mixer with 150mm centres, supplied with in-line STOP/CHECK connectors ideal for the needs of hospitals.

Chrome-plated brass body.

10-year warranty.