H9613

**SECURITHERM thermostatic sink mixer set**

Reference: H9613

Specification Description

SECURITHERM thermostatic sequential sink mixer and column with retracting hand spray.

Ideal for baby baths.

Anti-scalding failsafe: hot water shuts off immediately if cold water supply fails.

Securitouch thermal insulation prevents burns.

No risk of cross flow between the hot and cold water.

No non-return valves on the inlets.

Swivelling column H. 200mm L. 220mm.

Retracting hand spray with 2 jet options: flow straightener/rain effect.

Scale-resistant thermostatic sequential cartridge for single control temperature and flow-rate adjustment.

Temperature can be adjusted from cold water to 40°C with maximum temperature limiter set at 40°C.

Body with smooth interior.

Flow rate regulated at 7 lpm.

No manual contact thanks to Hygiene control lever L. 100mm.

Mixed water brass outlet L. 160mm.

BIOSAFE flexible shower hose reduces bacterial proliferation: transparent polyurethane, smooth interior and exterior, low water volume (internal Ø 6mm).

Specific counterweight.

PEX flexibles F3/8" and reinforced fixing via 2 stainless steel rods.

10-year warranty.