DELABIE_C100M35H963915

**SECURITHERM shower panel**

Reference: H963915

Specification Description

Aluminium powder-coated SECURITHERM sequential thermostatic shower panel for wall-mounted, exposed installation.

• Top inlets with M½" stopcocks.

•SECURITHERM sequential thermostatic mixer (non-time flow).

• Temperature control from cold water up to 39°C.

• Maximum temperature limiter set at 39°C, can be adjusted.

• Anti-scalding failsafe: hot water supply shuts-off immediately if cold water supply fails (and vice versa).

• Thermal shocks are possible.

• Flow rate 6 lpm at 3 bar.

• Chrome-plated ROUND shower head, tamperproof with scale-resistant nozzle with no grid and automatic flow rate regulator.

• Hygiene control lever L. 100mm.

Copper inlets.

• Concealed fixings and filters.