DELABIE_C100M35H9741TP

**SECURITHERM Securitouch thermostatic shower mixer**

Reference : H9741TP

CCTP description

Dual control SECURITHERM thermostatic shower mixer with:

- Anti-scalding safety: hot water shuts off immediately if cold water fails (and vice versa).

- Securitouch thermal insulation to prevent burns.

- Scale-resistant thermostatic cartridge for temperature adjustment.

- 1/4-turn ceramic head for flow rate adjustment.

- Adjustable temperature from 25°C to 41°C.

- Maximum temperature limiter pre-set to 38°C.

- Thermal shocks are easy to undertake without removing the control knob or shutting off the cold water.

- Flow rate regulated at 9 lpm.

- Chrome-plated brass body and ERGO controls.

- M1/2" shower outlet.

- Filters and non-return valves built-in to inlets M3/4".

Mixer with in-line STOP/PURGE connectors M1/2" M3/4" ideal for hospitals.