**Spare toilet roll holder with spindle**

Bright polished 304 stainless steel

Reference: **4070P**

Specification description

Wall-mounted toilet roll holder.

Spare toilet roll holder.

Bacteriostatic bright polished 304 stainless steel.

Tube Ø 25mm, 1.2 mm thick.

Concealed fixings.

30-year warranty.