**Wall-mounted pre-rinse set with mixer and telescopic spout**

With bib tap and swivelling telescopic spout

White flexible and scale-resistant spray

Reference: **G6432**

Specification description

Complete pre-rinse set with bib tap suitable for intensive use in professional kitchens.

Wall-mounted F3/4" mixer with 150mm centres with:

- valve heads with control knobs.

- non-return valves integrated in the mixer.

Bib tap with telescopic, swivelling spout L. 200-290mm.

- 20 lpm flow rate at the outlet.

- valve heads with control knobs.

White hand spray with adjustable jet with 9 lpm flow rate at the outlet (ref. 433000).

Scale-resistant hand spray with shock-resistant tip.

White, reinforced, food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.