**Recessed shower tray**

700 x 700mm

Reference: **150100**

Specification description

Recessed shower tray, 700 x 700mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

One-piece pressed shower tray, seam-free for easy maintenance and better hygiene.

Rounded internal corners for improved safety in the shower.

Drainage slope.

Supplied with 1½" waste.

Non-slip surface.

CE marked. Complies with European standard EN 14527.

Weight: 5.5kg.

[Formerly ref: 0513010000]