**Surgical scrub up trough with high splashback**

Polished satin 304 stainless steel - 1 service

With 2 tap holes Ø 22mm, centres 150mm

Reference: **181200**

Specification description

Wall-mounted surgical scrub up trough with splashback 360mm.

Suitable for hospitals and healthcare facilities.

L. 700mm, 1 service. With twin tap holes Ø 22 with 150mm centres.

Bacteriostatic 304 stainless steel. Stainless steel thickness: 1.5mm.

Smooth surface and rounded inside edges for easy cleaning.

Drainage on the right. Without overflow. Supplied with fixing elements.

CE marked. Complies with norm EN 14296.

Weight: 13.8kg.

30-year warranty.