**Soap dispenser specifically for showers**

For liquid soap

Watertight anodised aluminium cover

Reference: **510579**

Specification description

Soap dispenser for showers.

Specifically designed for showers: 100% waterproof, removes the risk of diluting the soap with water from the shower, maintaining the soap quality.

Push-button with soft-touch operation suitable for all users: children, people with reduced mobility etc.

Ergonomic push-button: large push-button, easy to press with wet hands or with an elbow.

Corrosion-resistant, waterproof, anodised aluminium cover.

Plastic tank: removes the risk of the aluminium deteriorating due to contact with the soap.

Tank with large opening: easy to refill from large containers.

No-waste, non-drip (waterproof) pump dispenser.

Anti-blocking: single dose per press, even if the button is pressed for prolonged periods.

Window for monitoring soap level.

Vandal-resistant model, lid opening is concealed.

Concealed fixings.

Clean lines are easy to clean and maintain, and improve hygiene.

Sleek design associated with DELABIE's range of shower panels.

Capacity: 1 litre.

Dimensions: 64 x 140 x 284mm.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s.

Wall-mounted soap dispenser specifically designed for showers with a 30-year warranty.