**TEMPOSTOP 3 time flow basin tap**

Fixings reinforced with 3 stainless steel screws

Reference: **703001**

Specification description

Deck-mounted push-button basin tap:

Time flow ~7 seconds.

Pre-set flow rate 3 lpm at 3 bar, adjustable from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Chrome-plated brass body M½".

Fixing reinforced by back-nut with 3 stainless steel screws.

30-year warranty