**TEMPOSTOP 3 time flow basin tap**

Length 50mm

Wall-mounted, 1/2"

Reference: **703200**

Specification description

Wall-mounted push-button basin tap:

~7 seconds time flow.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated brass body M1/2".

30-year warranty.