**HYGIÉNA waste**

Pre-scored waste with concave grid

M1 1/4"

Reference: **611**

Specification description

Hygienic washbasin waste M1 1/4" with concave grid (no water retention).

Free flow, with no central screw (avoids scale deposits and reduces bacterial development).

Pre-scored waste: snap-off sections can be removed for models with overflow.

Polished chrome-plated brass grid, chrome-plated ABS body.

Can adapt to any material and size of washbasin or sink.

Can be tightened to a minimum of 1mm or maximum of 45mm.