**SPEEDJET high-speed hand dryer, with filters and drip tray**

Air pulse

Metallic grey

Reference: **510621**

Specification description

SPEEDJET metallic grey two-way air pulse hand dryer.

High speed electrical hand dryer: dries in 10 - 18 seconds.

Removable drip tray prevents any water dripping onto the wall or floor: easy to clean and service.

ON/OFF button: easy to service.

Anti-bacterial air filter and activated carbon air filter.

Automatic hand dryer, infrared detection.

Intelligent technology: stops automatically when hands are removed or after 18 seconds of drying.

LCD screen with animated user guide and automatic stand-by.

Brushless motor, no wear.

Energy saving: power 850W. No heating element.

220-240V~/50-60Hz.

Airflow: 42 l/second. Air speed: 310km/h.

Noise level: 75-80 dBA.

Dimensions: 250 x 292 x 650mm.

Weight: 11.4kg.

Class I, IP22.

CE marked.

3-year warranty.