**Lift-up shower seat, with ALU leg**

Wall-mounted lift-up shower seat

White powder-coated aluminium structure

Reference: **510400**

Specification description

ALU lift-up shower seat with leg.

Shower seat for disabled people or people with reduced mobility.

Large plastic slats, comfortable and easy to maintain.

Folding leg guided by an articulated arm.

Structure made from white aluminium tube Ø 25mm x 2mm.

Concealed fixings.

Supplied with stainless steel screws for concrete walls.

Dimensions: 407 x 360 x 480mm.

Folded dimensions: 82 x 545mm.

Seat height: 480mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Wall-mounted lift-up with 30-year warranty. CE marked.