**Toilet paper dispenser for two rolls**

Bright polished 304 stainless steel

Reference: **1660**

Specification description

Wall-mounted toilet paper dispenser.

Twin toilet roll dispenser.

1 spare roll.

Vandal-resistant model.

With lock and standard DELABIE key.

Level control.

Toilet roll holder made from bacteriostatic bright polished 304 stainless steel.

Stainless steel thickness: 1mm.

Dimensions: 130 x 120 x 260mm.

30-year warranty.