**Toilet brush set**

Floor-standing model

304 stainless steel, polished satin

Reference: **4049S**

Specification description

Toilet brush set.

Robust toilet brush set.

Floor-standing model.

Bacteriostatic polished satin 304 stainless steel.

Easy to clean: plastic bowl can be removed from above.

Plastic bowl with reservoir: avoids toilet brush sitting in residual water and reduces the risk of splashing when next used.

Stainless steel thickness: 1mm body.

Dimensions: Ø 90 x 330mm.

30-year warranty.