**Toilet brush set with lid**

Floor-standing model

Polsihed satin 304 stainless steel

Reference: **4050S**

Specification description

Toilet brush set with lid.

Robust toilet brush set.

Floor-standing model.

Bacteriostatic polished satin 304 stainless steel.

Easy to clean: plastic bowl can be removed from above.

Plastic bowl with reservoir: avoids toilet brush sitting in residual water and reduces the risk of splashing when next used.

Toilet brush automatically centres itself in the holder.

Stainless steel thickness: 1mm.

Dimensions: Ø 90 x 410mm.

30-year warranty.