**Angled curtain rail**

Fixed

0.90 x 0.90 m

Reference: **1367**

Specification description

Angled curtain rail for showers

Bright polished 304 stainless steel angled rod, 1mm thick, for shower curtains.

Dimensions: Ø 20mm - 0.90 x 0.90m.

Concealed fixings.

30-year warranty.