**Basin or urinal waste**

With stainless steel grid

For basins or urinals

Reference: **580000**

Specification description

Basin or urinal waste:

Stainless steel grid Ø 63mm to cover a hole of Ø 54mm maximum.

Outlet M1¼".

Central screw.

30-year warranty.