**5-jet shower kit**

Ø 25mm rail

Reference: **803**

Specification description

Shower kit with 5 jets:

- chrome-plated stainless steel shower rail Ø 25mm, overall length 632mm with 602mm centres, can be cut to size,

- a sliding shower head holder, can be adjusted in height and inclined,

- chrome-plated soap dish,

- smooth, BICOLOR PVC flexible hose in food-grade metallo-plastic PVC, L. 1.50m (ref. 834T1),

- scale-resistant ABS chrome-plated shower head with 5 jets: rain effect, massage effect, bubbles, massage and rain effect, bubbles and rain effect (ref. 813)

- shower hose retaining collar (ref. 830).