**BICOLOR flexible shower hose**

Smooth PVC flexible hose FF1/2"

L. 0.85m

Reference: **834T3**

Specification description

Smooth, metalloplastic food grade PVC, BICOLOR flexible shower hose, FF1/2", L. 0.85m.

Easy to maintain and limits bacterial retention.

Thick PVC hose reinforced by thread polyester conforms to European standard EN 1113.

Food grade PVC inner tube.

Chrome-plated, conical brass connectors 1/2".

Will withstand strain (50kg), bending and twisting.