**Single hole mixer - 100 lpm**

Mixer with extension column with spout H.650 L.300

Mixer with high flow rate for plunge sinks

Reference: **5612**

Specification description

Deck-mounted, single hole mixer for professional kitchens.

Mixer for professional kitchens with extension column for installation on a stove top.

Mixer for plunge sinks with swivelling, tubular spout H. 650mm L. 300mm.

Star-shaped, brass flow straightener with smooth interior.

Water-free guided valve heads with reinforced mechanisms.

Shock-resistant, ergonomic ball levers.

Flow rate 100 lpm at 3 bar.

Full flow rate within half a turn.

Chrome-plated brass body and spout.

Soldered copper pipe water inlets.

Single hole mixer with reinforced fixings.

Mixer suitable for intensive use in professional kitchens.

Mixer for professional kitchens with 30-year warranty.