**Pre-rinse set with mixer**

With bib tap and telescopic spout

White flexible hose and scale-resistant hand spray

Reference: **6692**

Specification description

Complete pre-rinse set with bib tap suitable for intensive use in professional kitchens.

Deck-mounted single hole mixer with slimline control lever.

Supplied with F3/8" flexibles and non-return valves.

Bib tap with telescopic, swivelling spout L. 200 - 290mm.

- flow rate 16 lpm at the outlet.

- valve head with control knob.

White hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433000).

Scale-resistant hand spray with shock-resistant tip.

Reinforced, food-grade, white flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.