**MONOFOOT instant shut-off tap**

Pedal-operated

Floor-mounted

Reference: **736101**

Specification description

Foot-operated basin valve with instant flow:

Instant automatic shut-off.

Pedal can be raised for cleaning the floor.

Adjustable pedal height.

Fixing with 4 screws.

Filter.

Cold or mixed water supply.

Floor-mounted M½"

30-year warranty.