**TEMPOSTOP time flow shower kit**

Time flow

Exposed, chain-pull, adjustable GYM COMFORT head

Reference: **747004**

Specification description

Ceiling mounted chain-pull time flow shower kit:

TEMPOSTOP M½" time flow valve for mixed water, top supply.

For ceiling mounting.

Time flow ~15 seconds.

Flow rate 9 lpm at 3 bar, can be adjusted.

Chrome-plated solid brass body.

Lever and chain fitted with handle.

With adjustable, scale-resistant shower head GYM COMFORT.

30-year warranty.