**SIPHURINOIR**

Siphon with vertical outlet

Chrome-plated brass

Reference: **310000**

Specification description

Urinal vertical siphon Ø 50mm with compression seal.

Outlet Ø 32mm with nut.

Water level 50mm.

Chrome-plated brass.

30-year warranty.