**Urinal outlet to seal**

For sealing

1¼"

Reference: **775000**

Specification description

Urinal outlet for sealing.

Inlet Ø 54mm.

Outlet M 1¼".

Chrome-plated brass.

30-year warranty.