**Scale-resistant aerator**

F22/100

20 - 25 lpm, 5 units

Reference: **22.5P**

Specification description

Scale-resistant aerator without economiser.

F22/100.

Flow rate 20-25 lpm at 3 bar.

Supplied in packs of 5.