**Tilting mirror with long ergonomic lever**

Bright white HR Nylon lever

Reference: **510201N**

Specification description

Wall-mounted, rectangular, tilting mirror with long ergonomic lever which facilitates adjustment of mirror angle from a sitting position or by wheelchair users.

For disabled washrooms and combined installation: can be used from sitting, for people with reduced mobility, or standing position.

Quick and easy to install: just clip into place.

Anti-theft lock.

Tilting mirror with bright white HR Nylon lever

6mm thick safety glass mirror.

Mirror dimensions: 500 x 600mm.

Can be tilted up to 20°.

Tilting mirror with 30-year warranty.