**Recessed liquid soap dispenser, 1 litre**

For recessed installation

Polished satin 304 stainless steel

Reference: **510711S**

Specification description

Wall-mounted soap dispenser for recessed installation.

Liquid soap dispenser made from polished satin bacteriostatic 304 stainless steel.

Locking door with standard DELABIE key.

Plastic tank.

Concealed fixings.

Capacity: 1 litre.

Stainless steel 1.2mm thick.

Dimensions: 107 x 245 x 150mm.

For chlorine-free and pH neutral soap.

Compatible with hydroalcoholic gel.

Wall-mounted soap dispenser with 30-year warranty.