**BAILA floor-standing washbasin**

Polished satin 304 stainless steel

With central tap hole Ø 35mm

Reference: **121170**

Specification description

Floor-standing washbasin, height 830mm. Basin internal diameter: 310mm.

Design-led styling.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.8mm.

Rounded edges prevent injury.

With central tap hole Ø 35mm.

Supplied with 1¼" waste. Without overflow.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 12kg

30-year warranty.

[Formerly ref: 0210170008]