**Surgical scrub up trough with low splashback**

Polished satin 304 stainless steel - 2 services

With no tap hole

Reference: **182020**

Specification description

Wall-mounted surgical scrub up trough with splashback 75mm.

Suitable for hospitals and healthcare facilities.

Bacteriostatic 304 stainless steel. Polished satin finish. Stainless steel thickness: 1.2mm.

L. 1,400mm, 2 services. With no tap hole.

Smooth surface and rounded inside edges for easy cleaning.

Drainage on the right. Without overflow. Supplied with fixing elements.

CE marked. Complies with norm EN 14296

Weight: 18.8kg.

30-year warranty.