**Wall-mounted plaster sink**

Polished satin 304 stainless steel

Reference: **180130**

Specification description

Wall-mounted plaster sink.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.5mm.

Smooth surface and flat edges for easy cleaning.

Suitable for hospitals, healthcare establishments and leisure centres.

Supplied with removable plaster basket with lid to filter plaster debris.

Can be installed in 2 ways: bowl on the right or bowl on the left.

Waste outlet 1½".

Supplied with fixing elements. Weight: 17kg.

30-year warranty.

[Formerly ref: 0711130000]