**Basic angled grab bar 135°, satin, 400 x 400mm**

Polished satin 304 stainless steel, 3 fixing points

Ø 32mm

Reference: **35082S**

Specification description

Basic angled grab bar 135°, Ø 32mm, for people with reduced mobility.

Grab bar made from polished satin 304 stainless steel.

3 fixing points prevent the hand from getting trapped and simplify installation.

Concealed fixings, secured to wall by 3-hole stainless steel plate.

Dimensions: 400 x 400mm.

30-year warranty.

CE marked.