**Twin toilet roll holder**

For rolls

Polished satin 304 stainless steel

Reference: **510082S**

Specification description

Wall-mounted toilet roll holder.

Toilet roll holder for 2 rolls.

Tube Ø 20mm, 1mm thick.

Polished satin bacteriostatic 304 stainless steel.

Concealed fixings.

30-year warranty.