**Black pre-rinse set with no valve**

With bib tap and swivelling tubular spout

Black flexible and scale-resistant hand spray

Reference: **433622**

Specification description

Black pre-rinse set without valve suitable for intensive use in professional kitchens.

Bib tap with swivelling, tubular spout L. 200mm.

- full flow rate achieved within 1/4-turn.

- valve head with reinforced mechanism with ergonomic control.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433010).

Scale-resistant hand spray with shock-resistant tip.

Black reinforced food-grade flexible hose L. 0.95m.

3/4" short brass column for wall-mounted water control valve.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.

This pre-rinse set, with no water control valve, comprises spare parts for repairing pre-rinse sets.