**Toilet roll holder for grab bars, chrome-plated**

Chrome-plated ABS

Reference: **510081P**

Specification description

Toilet roll holder for grab bars.

Chrome-plated ABS.

Can be added without removing the grab bar.

Locks in place to prevent theft.

Anti-rotation locking feature.

Toilet roll holder for Ø 32mm bars.

30-year warranty.