**BINOPTIC wall-mounted electronic soap dispenser**

Liquid or foam soap dispenser

Mains, matte black 304 stainless steel, tube 1.2m

Reference: **512151BK**

Specification description

Wall-mounted electronic soap dispenser.

Liquid or foam soap dispenser.

No manual contact: infrared cell detects hands automatically.

Matte black 304 stainless steel spout.

No waste dose dispenser.

Separate electronic unit for installation beneath the washbasin.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with maximum viscosity of 3,000 mPa.s or specific foam soap.

Total spout length: 115mm.

Supplied with 1.20m flexible tube for remote tanks.

Wall-mounted electronic soap dispenser with 30-year warranty.

CE marked.