**Ø35mm ceramic cartridge**

Cartridge with base

With flow rate limiter

Reference: **N222**

Specification description

Ø35mm standard ceramic cartridge with base, with flow rate limiter.

For deck-mounted basin mixer ranges:

- 2220, 2220L / 2221, 2221L

- 25061T1, 2506T1

- 2720L, 2720T / 2721L, 2721T (for models sold since 12/2022)

- 2820L, 2820T (for models sold since 05/2023)