**Detector**

For TEMPOMATIC WC

4m cable

Reference: **463399**

Specification description

Detector.

For electronic TEMPOMATIC WC.

With cable: length 4m.