**Mechanical shower panel**

Mechanical, inlet via flexible

Removable shower head, aluminium

Reference: **791360**

Specification description

Mechanical shower panel:

Anodised aluminium panel for wall-mounted, exposed installation.

Non-time flow mechanical shower mixer.

Sliding shower head on chrome-plated rail with flexible.

Concealed inlet via flexible hoses.

M½" connections.

Concealed fixings.

Filters.

Shower panel suitable for people with reduced mobility.

30-year warranty.